**Analýzy – archeologická mapa**

1. Propojení s vodními toky – buffery kolem vodních toků, např. 100:100:1000 m a zjišťovat počet nálezů
2. Propojení se sídly – stejný princip jako v 1)
3. Zkusit propojení s nadmořskými výškami, histogram hodnot výšek všech nálezů
4. Vztah nálezů a kvality zemědělské půdy
5. Spojení s těžbou nerostných surovin

1.

Current buffer zone: [ 0m - 100m]; Amout of archeology spots: 21697

Current buffer zone: [100m - 200m]; Amout of archeology spots: 24378

Current buffer zone: [200m - 300m]; Amout of archeology spots: 18986

Current buffer zone: [300m - 400m]; Amout of archeology spots: 15155

Current buffer zone: [400m - 500m]; Amout of archeology spots: 10555

Current buffer zone: [500m - 600m]; Amout of archeology spots: 8489

Current buffer zone: [600m - 700m]; Amout of archeology spots: 6890

Current buffer zone: [700m - 800m]; Amout of archeology spots: 6039

Current buffer zone: [800m - 900m]; Amout of archeology spots: 5544

Current buffer zone: [900m - 1000m]; Amout of archeology spots: 4620

Total: 122353